status / chassis0 / slots / [SLOT-ID] / [rel1000] / module / ports / port[ID] / status
CLI REST-API

## mrs-flags

The submenu mrs-flags (mrs-flags) contains the following:
Menus: none
Objects:
is-supported (ref type cfg'd for this level is supported)
is-connected (input signal is connected)
signal-available (input signal available)
is-master (reference is master source)
is-locked (locked to input signal)
is-accurate (oscillator control has reached full accuracy)
is-settled (reference time signal settled)
is-phase-locked (oscillator phase locked to PPS)
num-src-exc (number of available sources exceeds what can be handled)
is-external (this ref source is on extension card)
low-jitter (this ref source has low jitter)
itu-limit-violated (ITU limits violated)
trs-limit-violated (Trusted source offset limit violated)
mttf-limit-violated (Max. time offset after sync. limit has been hit)
Commands: none

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CES
See also:
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-supported
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-connected
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/signal-available
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-master
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-locked
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-accurate
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-settled
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-phase-locked
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/num-src-exc
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/is-external
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/low-jitter
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/itu-limit-violated
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/trs-limit-violated
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status/mrs-flags/mttf-limit-violated

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ports/port.*/status/mrs-flags
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ports/port.*/status/mrs-flags