status / chassis0 / slots / [SLOT-ID] / [gln170] / module
CLI REST-API

## gln

The submenu gln (gln) contains the following:
Menus:
antenna (antenna status)
receiver (status of receiver)
Objects:
ref-type (ref-type)
receiver-status (receiver status)
Commands: none

#### Applies to modules

GLN170
See also:
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/gln/antenna
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/gln/receiver
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/gln/ref-type
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/gln/receiver-status

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/gln
Example using curl:

    curl /api/status/chassis0/slots/.*/module/gln