configuration / chassis0 / slots / [SLOT-ID] / [cpc200] / module / ports / port[ID]
CLI REST-API

## ltc-out-flags

The submenu ltc-out-flags (ltc-out-flags) contains the following:
Menus: none
Objects:
itu-r-br-1353 (Date encoding according to ITU-R BR.1353)
parity-enabled (Enable parity encoding)
Commands: none

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CES
See also:
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/ltc-out-flags/itu-r-br-1353
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/ltc-out-flags/parity-enabled

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ports/port.*/ltc-out-flags
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ports/port.*/ltc-out-flags

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ports/port.*/ltc-out-flags
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ports/port.*/ltc-out-flags
    -d "{
      \"objects\": \"new-values\"
    }"