configuration / network / general
CLI REST-API

## bonding-mode

Bonding-Mode
This is a read-write object and valid values are:

- active-backup [0]
- lacp [1]

See also:
/configuration/network/general: General Information
/configuration/network/general/hostname: Hostname
/configuration/network/general/domainname: Domainname
/configuration/network/general/nameserver-1: Nameserver 1
/configuration/network/general/nameserver-2: Nameserver 2
/configuration/network/general/ipv4-gateway: IPv4 Gateway
/configuration/network/general/ipv6-gateway: IPv6 Gateway
/configuration/network/general/cluster-port: Cluster Port
/configuration/network/general/cluster-multicast: Cluster IPv6 Multicast Address
/configuration/network/general/cluster-ipv6-port: Cluster IPv6 Port
/configuration/network/general/cluster-ipv6-multicast: Cluster IPv6 Multicast Address
/configuration/network/general/dscp-ntp: DSCP NTP Classification
/configuration/network/general/syslog-pingcheck: System-Log Pingcheck
/configuration/network/general/enable-alternate-prio1: enable alternate priority 1
/configuration/network/general/alternate-priority1: alternate priority1
/configuration/network/general/use-hps-card-slot-id: use hps card slot id

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/network/general
Example using curl:

    curl /api/configuration/network/general

Method: PATCH
URL: /api/configuration/network/general
Body:

    {
      "bonding-mode": "active-backup"
    }

Example using curl:

    curl -X PATCH /api/configuration/network/general -d
    {
      "bonding-mode": "active-backup"
    }