configuration / chassis0 / slots / [SLOT-ID] / [msf600] / module / ports / port[ID]
CLI REST-API

## gpio-type

gpio type
This is a read-only object and valid values are:

- fixed-pps [-1] (This is a PPS port)
- freq-in [0] (Variable frequency input, freq == 0 if input not used)
- freq-out [1] (Variable frequency output)
- fixed-freq-out [2] (Fixed frequency output)
- bits-in [3] (Framed data stream input)
- bits-out [4] (Framed data stream output)
- video-out [5] (Video signal output (PAL, NTSC, ...))
- video-sync-out [6] (Video sync signal output (H-Sync, V-Sync, ...))
- studio-clock-out [7] (Studio clock output)
- digital-audio-out [8] (Digital Audio output (DARS, ...))
- video-in [9] (Video signal input (PAL, NTSC, ...))
- ltc-out [10] (Linear Timecode output)
- ltc-in [11] (Linear Timecode input)
- gps [12] (GPS)
- frq [13] (10 MHz freq in)
- pps [14] (PPS in)
- 10mhz+pps [15] (10 MHz + PPS in)
- tcr [16] (IRIG)
- ntp [17] (NTP)
- ptp [18] (PTP (IEEE1588))
- ptp-e1 [19] (PTP over E1)
- fixed-freq-in [20] (Fixed Freq. in)
- string+pps [21] (PPS plus string)
- gpio [22] (Var. freq. via GPIO)
- reserved [23]
- pzf [24] (DCF77 PZF Receiver)
- lwr [25] (Long Wave Receiver)
- ggr [26] (GNSS Receiver)
- hqi [27] (HaveQuick Input)
- ext [28] (ext. Osc.)
- synce [29] (Synchronous Ethernet)

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CES
See also:
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/port-type
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/label
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/milli-phase
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/sa-bits
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/ssm
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/boc
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/vertical-offset
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/horizontal-offset
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/tc-line0
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/tc-line1
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/daily-jam
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/daily-jam-100th-sec
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/tc-line
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/channel
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/rcg-phase-offset
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/fixed-type
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/direction
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/op-mode
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/mrs-reference
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/ql-mask
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/hysteresis
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/discard-if-itu-violated
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/mode
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/tsu-port
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/gpio-type

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ports/port.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ports/port.*