configuration / ntp / multicast-cfg
CLI REST-API

## interval

Interval
This is a read-write object and valid values are:

- auto [0]
- 8 [8]
- 16 [16]
- 32 [32]
- 64 [64]
- 128 [128]
- 256 [256]
- 512 [512]
- 1024 [1024]

See also:
/configuration/ntp/broadcast-cfg/dummy: dummy
/configuration/ntp/broadcast-cfg/dummy/address: Address
/configuration/ntp/broadcast-cfg/dummy/use-autokey: Use Autokey
/configuration/ntp/broadcast-cfg/dummy/symmetric-key: Symmetric Key
/configuration/ntp/broadcast-cfg/dummy/ttl: TTL

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/ntp/multicast-cfg
Example using curl:

    curl /api/configuration/ntp/multicast-cfg

Method: PATCH
URL: /api/configuration/ntp/multicast-cfg
Body:

    {
      "interval": "auto"
    }

Example using curl:

    curl -X PATCH /api/configuration/ntp/multicast-cfg -d
    {
      "interval": "auto"
    }