status / chassis0 / slots / [SLOT-ID] / [scg] / module / ports
CLI REST-API

## port1

The submenu port1 (port1) contains the following:
Menus:
status (status)
Objects:
direction (direction)
port-type (port type)
fixed-type (fixed type)
mrs-reference (mrs-reference)
offset-ns (Offset in nanoseconds)
Commands: none

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CES
See also:
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/status
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/direction
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/port-type
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/fixed-type
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/mrs-reference
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/offset-ns
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ports/port.*
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ports/port.*