status / network / ports / lan[ID]
CLI REST-API

## card-name

name of the card
This is a read-only object and valid values are:

- unknown [0]
- lne_gb [53]
- lne180sfp [76]
- cpu [10001]
- c05f1 [20000]
- c05f1-v31 [20001]
- c05f1-v33 [20002]
- c05f1-v34 [20003]
- ims-c15g2 [20004]
- ims-c05f1 [20005]
- ims-cpu [20006]
- mbg-vma [20007]
- rx200s7 [20008]
- rx200s8 [20009]
- rx2530m1 [20010]
- dl325g10 [20011]
- ims_q7.b [20012]

See also:
/status/network/ports/lan[ID]
/status/network/ports/lan[ID]/port-available: port is available
/status/network/ports/lan[ID]/duplex
/status/network/ports/lan[ID]/operstate
/status/network/ports/lan[ID]/speed
/status/network/ports/lan[ID]/mac-address
/status/network/ports/lan[ID]/link
/status/network/ports/lan[ID]/slot-id: identification number of the slot, where the card is
/status/network/ports/lan[ID]/slot-name: name of the slot, where the card is
/status/network/ports/lan[ID]/port-id: port index of the card

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/network/ports/lan.*
Example using curl:

    curl /api/status/network/ports/lan.*