configuration / chassis0 / slots / [SLOT-ID] / [gns190] / module / mrs / ref
CLI REST-API

## max-correction-transition

Max Correction in Transition Mode
This is a read-write object and valid values are signed integers.
Datatype-Help:
value must be a signed number.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-time-deviation-follow
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-time-deviation-warmed-up
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-step-size-first-sync
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/ref/max-correction-warmed-up

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/mrs/ref
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/mrs/ref

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/mrs/ref
Body:

    {
      "max-correction-transition": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/mrs/ref -d
    {
      "max-correction-transition": 0
    }