status / network
CLI REST-API

## ports

The submenu ports (Physical Network Status) contains the following:
Menus:
lan0 (lan0)
Objects:
slot-id (identification number of the slot, where the card is)
slot-name (name of the slot, where the card is)
port-id (port index of the card)
port-available (port is available)
card-name (name of the card)
Commands: none
See also:
/status/network/ports/lan[ID]
/status/network/ports/slot-id: identification number of the slot, where the card is
/status/network/ports/slot-name: name of the slot, where the card is
/status/network/ports/port-id: port index of the card
/status/network/ports/port-available: port is available
/status/network/ports/card-name: name of the card
/configuration/network/ports: Physical Network Configuration

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/network/ports
Example using curl:

    curl /api/status/network/ports