configuration / chassis0 / slots / [SLOT-ID] / [bpe2352] / module / io-ports / port[ID]
CLI REST-API

## port-type

port type
This is a read-only object and valid values are:

- none [-1]
- fixed [0]
- configurable [1]

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CES
See also:
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/io-ports/port[ID]
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/io-ports/port[ID]/direction
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/io-ports/port[ID]/signal-type
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/io-ports/port[ID]/operation-mode
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/io-ports/port[ID]/signal-source

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/io-ports/port.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/io-ports/port.*