configuration / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / gps / serial-ports / com[ID]
CLI REST-API

## string-type

String Type
This is a read-write object and valid values are:

- none [-1]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/baudrate
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/framing
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/mode

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Body:

    {
      "string-type": "none"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.* -d
    {
      "string-type": "none"
    }