configuration / chassis0 / slots / [SLOT-ID] / [gns190] / module / gps
CLI REST-API

## serial-ports

The submenu serial-ports (Serial-Ports) contains the following:
Menus:
com0 (com0)
com1 (com1)
Objects: none
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps/serial-ports

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps/serial-ports
    -d "{
      \"objects\": \"new-values\"
    }"