status / chassis0 / slots / [SLOT-ID] / [lne_gb] / module / ports / port[ID]
CLI REST-API

## fixed-type

fixed type
This is a read-only object and valid values are:

- none [-1]
- gps [0] (GPS)
- frq [1] (10 MHz freq in)
- pps [2] (PPS in)
- 10mhz+pps [3] (10 MHz + PPS in)
- tcr [4] (IRIG)
- ntp [5] (NTP)
- ptp [6] (PTP (IEEE1588))
- ptp-e1 [7] (PTP over E1)
- fixed-freq [8] (Fixed Freq. in)
- string+pps [9] (PPS plus string)
- gpio [10] (Var. freq. via GPIO)
- reserved [11]
- pzf [12] (DCF77 PZF Receiver)
- lwr [13] (Long Wave Receiver)
- ggr [14] (GNSS Receiver)
- hqi [15] (HaveQuick Input)
- ext [16] (ext. Osc.)
- synce [17] (Synchronous Ethernet)
- video-in [18] (Video Input)
- ltc [19] (Linear Time Code)
- 10-mhz [20]
- 2048-khz [21]
- ethernet [22]
- terminal [23]
- prog-output [24]
- switch [25]
- timecode [26]
- light [27]
- antenna [28]
- uart [29]
- dcf77 [30]
- power [31]
- spst-relay [32]
- spdt-relay [33]
- synthesizer [34]
- multi [35]
- prog-output-1 [36]
- prog-output-2 [37]
- prog-output-3 [38]
- prog-output-4 [39]
- osc [40] (int. Osc.)

#### Applies to modules

GPS167
GPS167SV
PZF511
GPS170
TCR511
AM511
MSF511
GRC170
WWVB511
MGR170
PZF600
TCR600
GPS180
GLN170
MGR180
MSF600
WWVB600
ESI180
CPE180
LNO180
GRC180
LIU
MRI
BPE
RSC180
LNE_GB
SCG
FDM180
SPT
PZF180
REL1000
HPS100
VSG180
MSF180
WWVB180
CPC180
TCR180
LUE180
SCU_01
LNE180SFP
GTS180
GRC181
GNS181_UC
PSX210
CPC200
FDM180M
LSG180
GPS190
GNS181
PIO180
SSP100
VSI180
GNM181
RSC2000
REL1000_RC
VSG181
BPE2XXX
BPE2352
BPE8XXX
BPE6042
GNS190
CES
See also:
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/direction
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/port-type
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/mrs-reference
/status/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/offset-ns
/configuration/chassis0/slots/[SLOT-ID]/[am511]/module/ports/port[ID]/fixed-type

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ports/port.*
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ports/port.*