configuration / chassis0 / slots / [SLOT-ID] / [gns181] / module / mrs / xmulti / priority / priority[ID]
CLI REST-API

## limit

Limit-Of-Refclk
This is a read-write object and valid values are signed integers.
Datatype-Help:
value must be a signed number.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/type
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/fix-offset
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/precision

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*
Body:

    {
      "limit": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.* -d
    {
      "limit": 0
    }