status / chassis0 / slots / [SLOT-ID] / [gps190] / module
CLI REST-API

## gps

The submenu gps (gps) contains the following:
Menus:
antenna (antenna status)
receiver (status of receiver)
Objects:
ref-type (ref-type)
receiver-status (receiver status)
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/antenna
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/receiver
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/ref-type
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/receiver-status
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/gps
Example using curl:

    curl /api/status/chassis0/slots/.*/module/gps