configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / global
CLI REST-API

## profile-specific-extension

profile-specific-extension
This is a read-write object and valid values are:

- none [0]
- power-ieee-c37-238-2011 [1] (IEEE C37.238-2011 profile extension)
- telecom-itu-t-g-8265-1 [2] (ITU-T G.8265.1 profile extension)
- telecom-itu-t-g-8275-1 [3] (ITU-T G.8275.1 profile extension)
- smpte-st-2059-2 [4] (SMPTE ST 2059-2 profile extension)
- ieee-802-1as [5] (IEEE 802.1AS profile extension)
- utility-iec-61850-9-3 [6] (IEC/IEEE FDIS 61850-9-3 Power Utility profile extension)
- power-ieee-c37-238-2017 [8] (IEEE C37.238-2017 profile extension)

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/delay-mechanism
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/domain-number
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/timescale
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/priority-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/priority-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/sync-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/announce-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/delay-request-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-interval-duration
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-hybrid-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/profile-preset
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/network-protocol
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/announce-receipt-timeout
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-ip-address-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-ip-address-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-enable-alt-priority1-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/alt-priority2

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global
Body:

    {
      "profile-specific-extension": "none"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global -d
    {
      "profile-specific-extension": "none"
    }