configuration / chassis0 / slots / [SLOT-ID] / [gps170] / module / ppo / ppo[ID] / timer / timer[ID]
CLI REST-API

## on

on
This is a read-write object and valid values are daytimes.
Datatype-Help:
a daytime looks like this: HH:MM:SS.
HH is hours
MM is minutes
SS is seconds
Examples:
12:00:00
08:00:00
23:59:59
Some other Formats are also accepted.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/timer/timer[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/timer/timer[ID]/off

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*/timer/timer.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ppo/ppo.*/timer/timer.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*/timer/timer.*
Body:

    {
      "on": "23:59:59"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ppo/ppo.*/timer/timer.* -d
    {
      "on": "23:59:59"
    }