status / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / mrs / priority[SLOT-ID] / status / id
CLI REST-API

## type

type
This is a read-only object and valid values are:

- none [-1]
- gps [0] (GPS)
- frq [1] (10 MHz freq in)
- pps [2] (PPS in)
- 10mhz+pps [3] (10 MHz + PPS in)
- tcr [4] (IRIG)
- ntp [5] (NTP)
- ptp [6] (PTP (IEEE1588))
- ptp-e1 [7] (PTP over E1)
- fixed-freq [8] (Fixed Freq. in)
- string+pps [9] (PPS plus string)
- gpio [10] (Var. freq. via GPIO)
- reserved [11]
- pzf [12] (DCF77 PZF Receiver)
- lwr [13] (Long Wave Receiver)
- ggr [14] (GNSS Receiver)
- hqi [15] (HaveQuick Input)
- ext [16] (ext. Osc.)
- synce [17] (Synchronous Ethernet)
- video-in [18] (Video Input)
- ltc [19] (Linear Time Code)
- osc [20] (int. Osc.)

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/info/settings/id
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/info/settings/id/instance

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/mrs/priority.*/status/id
Example using curl:

    curl /api/status/chassis0/slots/.*/module/mrs/priority.*/status/id