configuration / chassis0 / slots / [SLOT-ID] / [gps167] / module / ppo / ppo[ID]
CLI REST-API

## length-s

length seconds
This is a read-write object and valid values are signed integers within a range of 0-59.
Datatype-Help:
value must be between 0 and 59.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/length-ms
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/output-level
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/output-holdover
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/mode
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/ppo/ppo[ID]/timeout

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ppo/ppo.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ppo/ppo.*
Body:

    {
      "length-s": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ppo/ppo.* -d
    {
      "length-s": 0
    }