configuration / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / gps / timezone / dst-off
CLI REST-API

## year

Year
This is a read-write object and valid values are years.
Datatype-Help:
value must be between 0 and 65534 or '****'.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/name
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/offset-sign
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/hour
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/minute
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/day
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/month
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/weekday
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/changing-hour
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/changing-minute
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/timezone/dst-off/changing-second

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps/timezone/dst-off
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps/timezone/dst-off

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps/timezone/dst-off
Body:

    {
      "year": "****"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps/timezone/dst-off -d
    {
      "year": "****"
    }