configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID]
CLI REST-API

## network

The submenu network (network) contains the following:
Menus: none
Objects:
net-link-mode (net-link-mode)
prp-mac-address-mode (PRP MAC Address Mode)
hostname (hostname)
domainname (domainname)
nameserver-0 (nameserver-0)
nameserver-1 (nameserver-1)
ipv4-address (ipv4-address)
ipv4-netmask (ipv4-netmask)
ipv4-gateway (ipv4-gateway)
ipv4-default-gateway (ipv4-default-gateway)
ipv6-mode (ipv6-mode)
ipv6-address (ipv6-address)
ipv6-gateway (ipv6-gateway)
ipv6-default-gateway (ipv6-default-gateway)
ipv6-multicast-scope (ipv6-multicast-scope)
dscp-ptp-classification (dscp-ptp-classification)
multicast-ttl (multicast-ttl)
dhcp-client (enable dhcp-client)
vlan-enabled (enable vlan option)
vlan-id (vlan-tag)
vlan-priority (priority)
Commands: none

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/net-link-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/prp-mac-address-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/hostname
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/domainname
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/nameserver-0
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/nameserver-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-address
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-netmask
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv4-default-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-address
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-default-gateway
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/ipv6-multicast-scope
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/dscp-ptp-classification
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/multicast-ttl
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/dhcp-client
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/vlan-enabled
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/vlan-id
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network/vlan-priority
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/network

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network
Body:

    {
      \"objects\": \"new-values\"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/network
    -d "{
      \"objects\": \"new-values\"
    }"