configuration / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / mrs / xmulti / priority / priority[ID]
CLI REST-API

## type

type
This is a read-write object and valid values are:

- none [0]
- gps [1]
- 10-mhz-freq-in [2]
- pps-in [3]
- 10-mhz-+-pps-in [4]
- irig [5]
- ntp [6]
- ptp-ieee1588 [7]
- ptp-over-e1 [8]
- fixed-freq-in [9]
- pps-plus-string [10]
- var-freq-via-gpio [11]
- dcf77-pzf-receiver [13]
- long-wave-receiver [14]
- gnss-receiver [15]
- havequick-input [16]
- ext-osc [17]
- synchronous-ethernet [18]
- video-input [19]
- linear-time-code [20]
- int-osc [21]
- string [22]
- hem [23]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/fix-offset
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/precision
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/xmulti/priority/priority[ID]/limit

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.*
Body:

    {
      "type": "none"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/mrs/xmulti/priority/priority.* -d
    {
      "type": "none"
    }