status / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / satellites / gnss / satellite-list / [ID]
CLI REST-API

## quality

quality
This is a read-only object and valid values are:

- no-signal [0] (No signal)
- searching-signal [1] (Searching signal)
- signal-acquired [2] (Signal acquired)
- signal-unusable [3] (Signal detected but unusable)
- code-locked [4] (Code locked and time synchronized)
- code-carrier-locked [5] (Code and carrier locked, and time synchronized)
- code-carrier-locked-2 [6] (Code and carrier locked, and time synchronized 2)
- code-carrier-locked-3 [7] (Code and carrier locked, and time synchronized 3)

#### Applies to modules

GPS167
GPS167SV
GPS170
GRC170
MGR170
GPS180
GLN170
MGR180
GRC180
GRC181
GNS181_UC
GPS190
GNS181
GNM181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/gnss-type
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/svno
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/cn-ratio
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/elevation
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/azimuth
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/pr-residual
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/selected
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/health
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/diff-correction-available
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/carrier-smoothed-pseudorange
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/orbit-source
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/ephemeris-parameters-available
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/almanac-parameters-available
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/assistnow-offline-available
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/assistnow-autonomous-available
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/sbas-corrections
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/rtcm-corrections
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/pseudorange-corrections
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/carrier-range-corrections
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/range-rate-corrections
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/in-use
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/authenticated
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gnss/satellite-list/[ID]/activated

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/satellites/gnss/satellite-list/.*
Example using curl:

    curl /api/status/chassis0/slots/.*/module/satellites/gnss/satellite-list/.*