configuration / chassis0 / slots / [SLOT-ID] / [gns190] / module / gps / serial-ports / com[ID]
CLI REST-API

## framing

Framing
This is a read-write object and valid values are:

- none [-1]
- 7n2 [0]
- 7e1 [1]
- 7e2 [2]
- 8n1 [3]
- 8n2 [4]
- 8e1 [5]
- 7o1 [6]
- 7o2 [7]
- 8o1 [8]
- 8e2 [9]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/baudrate
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/mode
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/serial-ports/com[ID]/string-type

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.*
Body:

    {
      "framing": "none"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps/serial-ports/com.* -d
    {
      "framing": "none"
    }