status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets / parent
CLI REST-API

## grandmaster-clock-quality

The submenu grandmaster-clock-quality (Quality of the grandmaster clock) contains the following:
Menus: none
Objects:
clock-class (PTP clock class representing the current sync status)
clock-accuracy (PTP clock accuracy)
log-variance (PTP offset scaled log variance representing the time stability)
Commands: none

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/grandmaster-clock-quality/clock-class
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/grandmaster-clock-quality/clock-accuracy
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/grandmaster-clock-quality/log-variance

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/parent/grandmaster-clock-quality
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/parent/grandmaster-clock-quality