status / chassis0 / slots / [SLOT-ID] / [tcr511] / module / irig
CLI REST-API

## timecode

The submenu timecode (timecode) contains the following:
Menus: none
Objects:
warmed-up (warmed up)
pulses-enabled (Pulses Enabled)
invalid-sysconf (Invalid Sysconf)
data-available (Data Available)
telegram-error (Telegram Error)
lock-on (Lock on)
tcap-exceed (TCAP Exceed)
invalid-utc-parm (Invalid UTC Parm)
Commands: none

#### Applies to modules

TCR511
TCR600
TCR180
See also:
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/warmed-up
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/pulses-enabled
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/invalid-sysconf
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/data-available
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/telegram-error
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/lock-on
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/tcap-exceed
/status/chassis0/slots/[SLOT-ID]/[tcr180]/module/irig/timecode/invalid-utc-parm

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/irig/timecode
Example using curl:

    curl /api/status/chassis0/slots/.*/module/irig/timecode