status / chassis0 / slots / [SLOT-ID] / [gns181] / module / gps
CLI REST-API

## ref-type

ref-type
This is a read-only object and valid values are:

- none [255]
- gps [0] (standard GPS)
- 10mhz-freqin [1] (10 MHz input frequency)
- pps-in [2] (1 PPS input signal)
- 10mhz-and-pps-in [3] (combined 10 MHz plus PPS)
- irig [4] (IRIG input)
- ntp [5] (Network Time Protocol)
- ptp-ieee1588 [6] (Precision Time Protocol)
- ptp-over-e1 [7] (PTP over E1)
- fixed-freq-in [8] (fixed frequency)
- pps-plus-string [9] (1 PPS in addition to time string)
- var-freq-via-gpio [10] (variable input signal via GPIO)
- unknown [11] (reserved, used internally by firmware only)
- dcf77-pzf-receiver [12] (DCF77 PZF providing much more accuracy than a standard LWR)
- long-wave-receiver [13] (long wave receiver. e.g. DCF77 AM, WWVB, MSF, JJY)
- gnss-receiver [14] (Glonass / GPS receiver)
- havequick-input [15] (HaveQuick input)
- ext-osc [16] (external oscillator disciplined and looped back via 1 PPS I/O)
- synchronous-ethernet [17] (Synchronous Ethernet, needs (external) ethernet interface)
- video-input [18] (Video In (Blackburst, VITC,...))
- linear-time-code [19] (Linear Time Code (Audio))
- int-osc [20] (internal Oscillator)
- string [21] (time string only)
- gnss [254]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/receiver-status

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/gps
Example using curl:

    curl /api/status/chassis0/slots/.*/module/gps