status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets / parent / grandmaster-clock-quality
CLI REST-API

## clock-accuracy

PTP clock accuracy
This is a read-only object and valid values are:

- no-accuracy [0]
- less-than-25ns [32]
- less-than-100ns [33]
- less-than-250ns [34]
- less-than-1000ns [35]
- less-than-2500ns [36]
- less-than-10us [37]
- less-than-25us [38]
- less-than-100us [39]
- less-than-250us [40]
- less-than-1000us [41]
- less-than-2500us [42]
- less-than-10ms [43]
- less-than-25ms [44]
- less-than-100ms [45]
- less-than-250ms [46]
- less-than-1s [47]
- less-than-10s [48]
- more-than-10s [49]
- unknown [254]

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/grandmaster-clock-quality
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/grandmaster-clock-quality/clock-class
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/grandmaster-clock-quality/log-variance

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/parent/grandmaster-clock-quality
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/parent/grandmaster-clock-quality