status / network / ports
CLI REST-API

## lan0

The submenu lan0 (lan0) contains the following:
Menus:
statistics (statistics)
Objects:
port-available (port is available)
duplex (duplex)
operstate (operstate)
speed (speed)
mac-address (mac-address)
link (link)
slot-id (identification number of the slot, where the card is)
slot-name (name of the slot, where the card is)
port-id (port index of the card)
card-name (name of the card)
Commands: none
See also:
/status/network/ports/lan[ID]/statistics
/status/network/ports/lan[ID]/port-available: port is available
/status/network/ports/lan[ID]/duplex
/status/network/ports/lan[ID]/operstate
/status/network/ports/lan[ID]/speed
/status/network/ports/lan[ID]/mac-address
/status/network/ports/lan[ID]/link
/status/network/ports/lan[ID]/slot-id: identification number of the slot, where the card is
/status/network/ports/lan[ID]/slot-name: name of the slot, where the card is
/status/network/ports/lan[ID]/port-id: port index of the card
/status/network/ports/lan[ID]/card-name: name of the card
/configuration/network/ports/lan[ID]

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/network/ports/lan.*
Example using curl:

    curl /api/status/network/ports/lan.*