configuration / network / interfaces / vif[ID] / ipv6
CLI REST-API

## ip-address

tcp/IP address
This is a read-write object and valid values are IPv6-addresses.
Datatype-Help:
the ipv6-address should looks like this: AAAA:BBBB:CCCC:DDDD:EEEE:FFFF:GGGG:HHHH/I
letters A - H are hex-digits.
valid hex-digits are: 0-9 and a-f.
letter I is a decimal number that goes from 0 to 128 and is a subnetmask.
example: 2001:0db8:85a3:08d3:1319:8a2e:0370:7344/64
See also:
/configuration/network/interfaces/vif[ID]/ipv6
/configuration/network/interfaces/vif[ID]/ipv6/gateway
/configuration/network/interfaces/vif[ID]/ipv6/enable-dhcp
/configuration/network/interfaces/vif[ID]/ipv6/dhcp-client-id

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/network/interfaces/vif.*/ipv6
Example using curl:

    curl /api/configuration/network/interfaces/vif.*/ipv6

Method: PATCH
URL: /api/configuration/network/interfaces/vif.*/ipv6
Body:

    {
      "ip-address": "::"
    }

Example using curl:

    curl -X PATCH /api/configuration/network/interfaces/vif.*/ipv6 -d
    {
      "ip-address": "::"
    }