configuration / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / gps
CLI REST-API

## enable-pulses

Enable Pulses
This is a read-write object and valid values are:

- if-sync [0]
- always [1]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/antenna-cable-length
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/ignore-lock
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/time-scale
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/enable-serial
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/enable-synth
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/synth-frequency
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/synth-range
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/synth-phase
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/irig-code
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/irig-mode

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps
Body:

    {
      "enable-pulses": true
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps -d
    {
      "enable-pulses": true
    }

Valid values when accessing this object via REST API/JSON: false [0], true [1]