status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets / port
CLI REST-API

## log-sync-interval

mean sync interval to be used for multicast messages
This is a read-only object and valid values are:

- 1/128 [-7]
- 1/64 [-6]
- 1/32 [-5]
- 1/16 [-4]
- 1/8 [-3]
- 1/4 [-2]
- 1/2 [-1]
- 1/1 [0]
- 2/1 [1]
- 4/1 [2]
- 8/1 [3]
- 16/1 [4]
- 32/1 [5]
- 64/1 [6]
- 128/1 [7]

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/port-state
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/log-min-delay-req-interval
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/log-announce-interval
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/announce-receipt-timeout
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/delay-mechanism
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/log-min-pdelay-req-interval
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/port/version-number

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/port
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/port