status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets / parent
CLI REST-API

## parent-port-identity

The submenu parent-port-identity (Identity of the master port, that issues the sync messages) contains the following:
Menus: none
Objects:
clock-identity (PTP clock identity)
port-number (PTP port ID)
Commands: none

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/parent-port-identity/clock-identity
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/parent/parent-port-identity/port-number

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/parent/parent-port-identity
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/parent/parent-port-identity