configuration / chassis0 / slots / [SLOT-ID] / [gns190] / module / tcr
CLI REST-API

## irig-code

IRIG Code
This is a read-write object and valid values are:

- b122-b123 [0] (100 bps, 1 kHz carrier, SBS optionally)
- a132-a133 [1] (1000 bps, 10 kHz carrier, SBS optionally)
- b002-b003 [2] (100 bps, DCLS, SBS optionally)
- a002-a003 [3] (1000 bps, DCLS, SBS optionally)
- afnor [4] (100 bps, 1 kHz carrier, complete date, SBS)
- afnor-dc [5] (100 bps, DCLS, complete date, SBS)
- ieee1344 [6] (100 bps, 1 kHz carrier, SBS, time zone info)
- ieee1344-dc [7] (100 bps, DCLS, SBS, time zone info)
- b126-b127 [8] (100 bps, 1 kHz carrier, 2 digit year number, SBS optionally)
- b006-b007 [9] (100 bps, DCLS, 2 digit year number, SBS optionally)
- g142 [10] (10 kbps, 100 kHz carrier)
- g002 [11] (10 kbps, DCLS)
- c37118 [12] (like IEEE1344, but UTC offset with reversed sign)
- c37118-dc [13] (like IEEE1344 DC, but UTC offset with reversed sign)
- txc101 [14] (code from TV time sync device TXC-101 DTR-6)
- txc101-dc [15] (DC code from TV time sync device TXC-101 DTR-6)
- e112 [16] (10 bps, 100 Hz carrier)
- e002 [17] (10 bps, DCLS)
- nasa36 [18] (100 bps, 1 kHz carrier)
- nasa36-dc [19] (100 bps, DCLS)
- a136-a137 [20] (1000 bps, 10 kHz carrier, 2 digit year number, SBS optionally)
- a006-a007 [21] (1000 bps, DCLS, 2 digit year number, SBS optionally)
- g146 [22] (10 kbps, 100 kHz carrier, 2 digit year number)
- g006 [23] (10 kbps, DCLS, 2 digit year number)

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-sign
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-hours
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/utc-offset-minutes
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/ignore-lock
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/enable-pulses
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-tfom-input
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/tcr/irig-tfom-output

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/tcr
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/tcr

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/tcr
Body:

    {
      "irig-code": "b122-b123"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/tcr -d
    {
      "irig-code": "b122-b123"
    }