configuration / ntp / multicast-cfg
CLI REST-API

## use-autokey

Use Autokey
This is a read-write object and valid values are:

- no [0]
- yes [1]

See also:
/configuration/ntp/broadcast-cfg/dummy: dummy
/configuration/ntp/broadcast-cfg/dummy/address: Address
/configuration/ntp/broadcast-cfg/dummy/interval: Interval
/configuration/ntp/broadcast-cfg/dummy/symmetric-key: Symmetric Key
/configuration/ntp/broadcast-cfg/dummy/ttl: TTL

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/ntp/multicast-cfg
Example using curl:

    curl /api/configuration/ntp/multicast-cfg

Method: PATCH
URL: /api/configuration/ntp/multicast-cfg
Body:

    {
      "use-autokey": true
    }

Example using curl:

    curl -X PATCH /api/configuration/ntp/multicast-cfg -d
    {
      "use-autokey": true
    }

Valid values when accessing this object via REST API/JSON: false [0], true [1]