status / chassis0 / slots / [SLOT-ID] / [gns190] / module / gns
CLI REST-API

## receiver-status

receiver status
This is a read-only object and valid values are:

- unknown [0]
- synchronized [1]
- tracking [2]
- no-antenna [3]
- warm-boot [4]
- cold-boot [5]
- short-circuit [6]

#### Applies to modules

GNS181_UC
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gns
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gns/ref-type

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/gns
Example using curl:

    curl /api/status/chassis0/slots/.*/module/gns