status / chassis0 / slots / [SLOT-ID] / [hps100] / module / sync-e
CLI REST-API

## output-ssm

output-ssm
This is a read-only object and valid values are:

- ql-stu/ukn [0]
- ql-prs [1]
- ql-prc [2]
- ql-inv3 [3]
- ql-ssu-a/tnc [4]
- ql-inv5 [5]
- ql-inv6 [6]
- ql-st2 [7]
- ql-ssu-b [8]
- ql-inv9 [9]
- ql-eec2/st3 [10]
- ql-eec1/sec [11]
- ql-smc [12]
- ql-st3e [13]
- ql-prov [14]
- ql-dnu/dus [15]

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/sync-e-status
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/input-ssm
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/sync-e/gbit-link-status

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/sync-e
Example using curl:

    curl /api/status/chassis0/slots/.*/module/sync-e