status / chassis0 / slots / [SLOT-ID] / [gps167sv] / module / mrs / priority[SLOT-ID] / status
CLI REST-API

## soc

signal outage counter
This is a read-only object and valid values are unsigned integers within a range of 0-255.

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/mrs-status
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/offset
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/ssm

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/mrs/priority.*/status
Example using curl:

    curl /api/status/chassis0/slots/.*/module/mrs/priority.*/status