status / chassis0 / slots / [SLOT-ID] / [gps190] / module / mrs / priority[SLOT-ID]
CLI REST-API

## status

The submenu status (status) contains the following:
Menus:
id (id)
mrs-flags (mrs-flags)
flags (flags)
Objects:
mrs-status (mrs-status)
offset (time offset from main time base)
ssm (synchronization status message)
soc (signal outage counter)
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
PZF180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/id
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/mrs-flags
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/flags
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/mrs-status
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/offset
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/ssm
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/mrs/priority[SLOT-ID]/status/soc

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/mrs/priority.*/status
Example using curl:

    curl /api/status/chassis0/slots/.*/module/mrs/priority.*/status