configuration / chassis0 / slots / [SLOT-ID] / [gps190] / module / gps
CLI REST-API

## irig-code

IRIG Code
This is a read-write object and valid values are:

- b002-b122 [0] (100 bps, DCLS or 1 kHz carrier)
- b003-b123 [1] (100 bps, DCLS or 1 kHz carrier, SBS)
- a002-a132 [2] (1000 bps, DCLS or 10 kHz carrier)
- a003-a133 [3] (1000 bps, DCLS or 10 kHz carrier, SBS)
- afnor [4] (100 bps, DCLS or 1 kHz carrier, complete date, SBS)
- ieee1344 [5] (100 bps, DCLS or 1 kHz carrier, 2 digit year number, SBS, UTC offset, DST and Leapsec status)
- b2201344 [6] (100 bps, Manchester enc., DCLS only, 2 digit year number, SBS, UTC offset, DST and Leapsec status)
- b222 [7] (100 bps, Manchester enc., DCLS only)
- b223 [8] (100 bps, Manchester enc., DCLS only, SBS)
- b006-b126 [9] (100 bps, DCLS or 1 kHz carrier, 2 digit year number)
- b007-b127 [10] (100 bps, DCLS or 1 kHz carrier, 2 digit year number, SBS)
- g002-g142 [11] (10 kbps, DCLS or 100 kHz carrier)
- g006-g146 [12] (10 kbps, DCLS or 100 kHz carrier, 2 digit year number)
- c37118 [13] (100 bps, DCLS or 1 kHz carrier, 2 digit year number, SBS, UTC offs. reverse to 1344, DST/Leapsec status)
- txc101 [14] (code from TV time sync device TXC-101 DTR-6)
- e002-e112 [15] (10 bps, DCLS or 100 Hz carrier)
- nasa36 [16] (100 bps, DCLS or 1 kHz carrier)
- a006-a136 [17] (1000 bps, DCLS or 10 kHz carrier, 2 digit year number)
- a007-a137 [18] (1000 bps, DCLS or 10 kHz carrier, 2 digit year number, SBS)
- b000-b120 [19] (100 bps, DCLS or 1 kHz carrier, SBS, control functions (CF) customer defined)
- b001-b121 [20] (100 bps, DCLS or 1 kHz carrier, control functions (CF) customer defined)

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/antenna-cable-length
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/ignore-lock
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/time-scale
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/enable-pulses
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/enable-serial
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/enable-synth
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/synth-frequency
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/synth-range
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/synth-phase
/configuration/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/irig-mode

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/gps
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/gps

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/gps
Body:

    {
      "irig-code": "b002-b122"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/gps -d
    {
      "irig-code": "b002-b122"
    }