configuration / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / global
CLI REST-API

## announce-interval

used in MC Master or UC Slave mode
This is a read-write object and valid values are:

- 1/128 [-7]
- 1/64 [-6]
- 1/32 [-5]
- 1/16 [-4]
- 1/8 [-3]
- 1/4 [-2]
- 1/2 [-1]
- 1/1 [0]
- 2/1 [1]
- 4/1 [2]
- 8/1 [3]
- 16/1 [4]
- 32/1 [5]
- 64/1 [6]
- 128/1 [7]

#### Applies to modules

HPS100
See also:
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/delay-mechanism
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/domain-number
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/timescale
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/priority-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/priority-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/sync-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/delay-request-interval
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-interval-duration
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-hybrid-mode
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/profile-preset
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/network-protocol
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/announce-receipt-timeout
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/profile-specific-extension
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-ip-address-1
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-unicast-ip-address-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/ptp-enable-alt-priority1-2
/configuration/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/alt-priority2
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/global/announce-interval

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global
Example using curl:

    curl /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global

Method: PATCH
URL: /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global
Body:

    {
      "announce-interval": "1/128"
    }

Example using curl:

    curl -X PATCH /api/configuration/chassis0/slots/.*/module/ptpv2/instances/instance.*/global -d
    {
      "announce-interval": "1/128"
    }