status / chassis0 / slots / [SLOT-ID] / [grc180] / module / grc
CLI REST-API

## receiver-status

receiver status
This is a read-only object and valid values are:

- unknown [0]
- synchronized [1]
- tracking [2]
- no-antenna [3]
- warm-boot [4]
- cold-boot [5]
- short-circuit [6]

#### Applies to modules

GRC180
GRC181
See also:
/status/chassis0/slots/[SLOT-ID]/[grc180]/module/grc
/status/chassis0/slots/[SLOT-ID]/[grc180]/module/grc/ref-type

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/grc
Example using curl:

    curl /api/status/chassis0/slots/.*/module/grc