status / chassis0 / slots / [SLOT-ID] / [scu_01] / module
CLI REST-API

## scu-status

The submenu scu-status (scu-status) contains the following:
Menus: none
Objects:
time-sync-1 (state of time sync signal clk_1)
time-sync-2 (state of time sync signal clk_2)
is-auto-mode (AUTOMATIC/REMOTE or MANUAL Mode)
selected-clock (selected clock)
time-diff (time-diff)
Commands: none

#### Applies to modules

RSC180
SCU_01
RSC2000
See also:
/status/chassis0/slots/[SLOT-ID]/[rsc180]/module/scu-status/time-sync-1
/status/chassis0/slots/[SLOT-ID]/[rsc180]/module/scu-status/time-sync-2
/status/chassis0/slots/[SLOT-ID]/[rsc180]/module/scu-status/is-auto-mode
/status/chassis0/slots/[SLOT-ID]/[rsc180]/module/scu-status/selected-clock
/status/chassis0/slots/[SLOT-ID]/[rsc180]/module/scu-status/time-diff

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/scu-status
Example using curl:

    curl /api/status/chassis0/slots/.*/module/scu-status