status / chassis0 / slots / [SLOT-ID] / [gps167] / module / sync-status / clock-status
CLI REST-API

## oscillator

oscillator status
This is a read-only object and valid values are:

- not-warmed-up [0]
- not-applicable [-1]
- warmed-up [1]

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/sync-status/clock-status
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/sync-status/clock-status/clock

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/sync-status/clock-status
Example using curl:

    curl /api/status/chassis0/slots/.*/module/sync-status/clock-status