configuration / network / interfaces / vif[ID] / cluster / ipv4
CLI REST-API

## priority

priority
This is a read-write object and valid values are signed integers within a range of 0-10.
Datatype-Help:
value must be between 0 and 10.
See also:
/configuration/network/interfaces/vif[ID]/vlan
/configuration/network/interfaces/vif[ID]/vlan/enable-vlan
/configuration/network/interfaces/vif[ID]/vlan/vlan-id

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/network/interfaces/vif.*/cluster/ipv4
Example using curl:

    curl /api/configuration/network/interfaces/vif.*/cluster/ipv4

Method: PATCH
URL: /api/configuration/network/interfaces/vif.*/cluster/ipv4
Body:

    {
      "priority": 0
    }

Example using curl:

    curl -X PATCH /api/configuration/network/interfaces/vif.*/cluster/ipv4 -d
    {
      "priority": 0
    }