status / chassis0 / slots / [SLOT-ID] / [grc180] / module / satellites / gnss / satellite-list / [ID]
CLI REST-API

## gnss-type

gnss-type
This is a read-only object and valid values are:

- gps [0] (GPS, United States)
- glonass [1] (GLONASS, Russia)
- beidou [2] (BEIDOU, China)
- galileo [3] (GALILEO, Europe)
- waas [4] (WAAS, Wide Area Augmentation System)
- egnos [5] (EGNOS, European Geostationary Navigation Overlay Service)
- qzss [6] (QZSS, Quasi Zenith Satellite System)
- generic [7] (GENERIC, Satellite Data generated from String)
- sbas [8] (SBAS, Satellite Based Augmentation Systems)
- lband [9] (Atomichron, LBAND Inmarsat (Fugro Atomichron))

#### Applies to modules

GPS167
GPS167SV
GPS170
GRC170
MGR170
GPS180
GLN170
MGR180
GRC180
GRC181
GNS181_UC
GPS190
GNS181
GNM181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gln170]/module/satellites/gps

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/satellites/gnss/satellite-list/.*
Example using curl:

    curl /api/status/chassis0/slots/.*/module/satellites/gnss/satellite-list/.*