status / chassis0 / slots / [SLOT-ID] / [hps100] / module / ptpv2 / instances / instance[ID] / datasets / time-properties
CLI REST-API

## time-source

source of time used by the grandmaster clock
This is a read-only object and valid values are:

- no-source [0]
- atomic clock [16]
- gps [32]
- terrestrial radio [48]
- ptp [64]
- ntp [80]
- hand set [96]
- other [144]
- internal oscillator [160]

#### Applies to modules

HPS100
See also:
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/time-properties
/status/chassis0/slots/[SLOT-ID]/[hps100]/module/ptpv2/instances/instance[ID]/datasets/time-properties/current-utc-offset

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/time-properties
Example using curl:

    curl /api/status/chassis0/slots/.*/module/ptpv2/instances/instance.*/datasets/time-properties