status / chassis0 / slots / [SLOT-ID] / [gns181_uc] / module / gps
CLI REST-API

## receiver

The submenu receiver (status of receiver) contains the following:
Menus: none
Objects:
synchronized (synchronized)
tracking (tracking)
warm-boot (warm-boot)
cold-boot (cold-boot)
Commands: none

#### Applies to modules

GPS167
GPS167SV
GPS170
GPS180
GNS181_UC
GPS190
GNS181
GNS190
See also:
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/receiver/synchronized
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/receiver/tracking
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/receiver/warm-boot
/status/chassis0/slots/[SLOT-ID]/[gns181]/module/gps/receiver/cold-boot

#### REST-API Support:

This menu is supported by the REST API:
Method: GET
URL: /api/status/chassis0/slots/.*/module/gps/receiver
Example using curl:

    curl /api/status/chassis0/slots/.*/module/gps/receiver