configuration / network / interfaces / vif[ID] / misc
CLI REST-API

## label

label
This is a read-write object and valid values are strings with a length of 0-9.
Datatype-Help:
value must be a string.
the length must be between 0 and 9.
See also:
/configuration/network/interfaces/vif[ID]/misc
/configuration/network/interfaces/vif[ID]/misc/assigned-port

#### REST-API Support:

This object is supported by the REST API:
Method: GET
URL: /api/configuration/network/interfaces/vif.*/misc
Example using curl:

    curl /api/configuration/network/interfaces/vif.*/misc

Method: PATCH
URL: /api/configuration/network/interfaces/vif.*/misc
Body:

    {
      "label": "Meinberg"
    }

Example using curl:

    curl -X PATCH /api/configuration/network/interfaces/vif.*/misc -d
    {
      "label": "Meinberg"
    }